 1. Frequency
    10 - 10000 MHz

2. Port
    Port 1 - RF input
    Port 2 - Vdd2/Vd
    Port 3 - Vdd3/Vd RF output

3. Bias Condition
    Vcc  = 3.3, 4.2, 5.0
    Vbias(Venable1 & Venable2) = 3.3, 4.4, 5.0v
    Iccq - 33, 62, 90mA
 
4. General info
    - GRF5219 DC2513
    - -25dBm input power, 9991 points, 1MHz Step, Start 10M Stop 10000MHz
    - De-embedded to the EVB Device pads using port extension method (open and short)
    - Collected on 08/21/2026

5. Part Specific info
     -GRF5219 is a 3-Stage PA with external tunable interstage
     -3 port S-parameter file is needed to properly model part